{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Order Form","Tab2 - Series IV","Tab3 - Cargo Cover","Tab4 - Bottom Rail Heights"],"not_rendered":{"charts":0,"images":28,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Order Form","index":0,"n_rows":41,"n_cols":23,"rows_kept":41,"cut":false,"hidden":false,"merged":[[3,0,3,2],[8,0,8,14],[11,0,11,1],[10,0,10,1],[5,3,5,6],[5,0,5,2],[5,7,5,8],[6,3,6,12],[5,9,5,12],[11,2,11,7],[10,2,10,7],[9,0,9,7],[34,12,34,14],[32,1,32,11],[34,1,34,11],[31,1,31,11],[25,1,25,2],[28,1,28,11],[21,6,21,9],[22,6,22,9],[23,1,23,5],[22,1,22,5],[25,3,25,4],[25,5,25,14],[24,12,24,14],[29,1,29,11],[24,3,24,11],[0,13,0,14],[2,0,2,2],[7,0,7,14],[15,0,15,1],[1,13,1,14],[1,3,1,12],[0,3,0,12],[2,13,3,14],[4,13,4,14],[6,0,6,2],[4,0,4,2],[4,3,4,12],[3,3,3,12],[2,3,2,12],[37,0,38,14],[36,0,36,2],[26,12,26,14],[26,3,26,11],[31,12,31,14],[30,12,30,14],[28,12,28,14],[27,12,27,14],[35,12,35,14],[33,1,33,11],[33,12,33,14],[35,1,35,11],[32,12,32,14],[30,1,30,11],[29,12,29,14],[12,0,12,1],[27,1,27,11],[26,1,26,2],[24,1,24,2],[19,1,19,5],[20,1,20,5],[12,2,12,7],[21,1,21,5],[15,2,15,7],[14,2,14,7],[13,2,13,7],[19,6,19,9],[20,6,20,9],[14,0,14,1],[13,0,13,1],[23,6,23,9]]}
[null,null,null,"REPLACEMENT DOOR - CARGO COVER - PARTS",null,null,null,null,null,null,null,null,null,"800-827-3692"]
[null,null,null,"Order Form",null,null,null,null,null,null,null,null,null,"rom.orders@romcorp.com"]
["Cust. Name:",null,null,null,null,null,null,null,null,null,null,null,null,"For more information\nvisit our website:"]
["Address:"]
["City / State / Zip:",null,null,null,null,null,null,null,null,null,null,null,null,"www.romcorp.com"]
["Contact Name:",null,null,null,null,null,null,"Phone #:"]
["Contact Email:"]
["** PLEASE READ:  If the door to be replaced or the vehicle it is installed on was built prior to 1998 or it's a Series III door, \n    that model is no longer available.  The replacement R•O•M door and parts is our current Series IV model that is slightly \n    different in appearance.  One difference is the bottom rail of our current model, does not match the older model. **"]
["** If a new Bottom Rail replacement is needed & the original door was purchased prior to May-1998, \n   then a Current Side Seal will need to be purchased also.**"]
["PARTS NEEDED"]
["Qty",null,"ITEM # - for part #'s - see TABs 2-4 below"]
[]
[]
[]
[]
[]
[]
["To Build a suitable replacement - we need the following info:"]
[]
[1,"What is the Serial Number on the nameplate:"]
[2,"OEM / Manufacturer of vehicle door is installed on:"]
[3,"Year Vehicle was manufactured:"]
[4,"Slat Length (do not include Nylon End Shoes):\n(inches) (reference drawing to the right)"]
[5,"Track Length? (inches) (measure from top to bottom)"]
[6,"Finish Type:",null,"Brushed - horizontal lines milled into the aluminum color surface  /\nSatin - smooth aluminum color   /    Painted --- specify color in #7 below",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brushed","Satin","Painted"]
[7,"If painted:",null,"Specify the Color  -->"]
[8,"Roll Type:",null,"Front Roll rolls up just behind header or Rear Roll rolls up at back of compartment.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Front Roll","Rear Roll"]
[9,"Bottom Rail Height? (standard, tall bottom rail or bottom rail extension) (see illustrations on Tab 4)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Standard Bottom Rail","Tall Bottom Rail","Bottom Rail Extension"]
[10,"Bottom Rail Elastic Pull Strap needed: (20\" / 30\" / 40\")",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20\" Elastic Pull Strap \n(doors <35\" OH)","30\" Elastic Pull Strap \n(doors 35\"-65\" OH)","40\" Elastic Pull Strap \n(doors >65\" OH)","None"]
[11,"Manual or Power Lock: (if power lock - Left Side / Right Side / Both Sides)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Manual Lock","Power Lock - Left Side","Power Lock - Right Side","Power Locks - Both Sides"]
[12,"Type of Key for Door Lock:    (J-236  /  1250  /  751   /  none)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"J-236",1250,751,"None"]
[13,"Track Style used on your door: (reference cross section drawings below)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Conventional \n(Standard)","Recessed","Interior","Integrated \nwith Light","Interior Integrated \nwith Light"]
[14,"If selected Integrated track, do you need a replacement White or Red-White DuroStrip LED?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes - V5 White LED","Yes - V5 Red-Whte LED","No"]
[15,"DuroStripTM V5 LED location: (Left side / Right side / Both Sides, if both, 2 lights will be ordered)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Left Side","Right Side","Both Sides (2 lights)"]
[16,"DuroStripTM V5 LED wire lead location: (Exits the Top or Exits the Bottom)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wire Exits the Top","Wire Exits the Bottom"]
[17,"Is a Light Switch installed in one of the black nylon strike blocks at the bottom of the track:\n(Strike Blocks are the nylon hold down blocks that secure the lift bar / tube handle)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","No"]
["Comments:"]
[]
[]
[]
["R•O•M • 6800 East 163rd Street • Belton, MO 64012"]

{"sheet":"Tab2 - Series IV","index":1,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["R•O•M Roll-up Shutter Door Parts Manual - FM-8.5-118  (click to download a copy of the parts manual)"]
["SERIES IV specific pages from the Parts Manual"]

{"sheet":"Tab3 - Cargo Cover","index":2,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["R•O•M Cargo Cover Parts Manual - FM-8.5-53 - Rev G - 10-18-2023  (click to download a copy of the parts manual)"]
["CARGO COVER specific pages from the Parts Manual"]

{"sheet":"Tab4 - Bottom Rail Heights","index":3,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["SERIES IV - BOTTOM RAIL HEIGHTS"]
[]
["·","STANDARD BOTTOM RAIL"]
[]
["·","TALL BOTTOM RAIL - This single piece option adds approximately 1-1/2\" of additional clearance between the lift bar and threshold.  \nThis option is best used when a compartment’s threshold extends beyond the vertical plane of the curtain’s outer surface."]
[]
["·","BOTTOM RAIL EXTENSION – This dual piece option adds ½” of additional clearance between the lift bar and the threshold.  \nThis option is best used when a compartment threshold extends beyond the vertical plane of the curtain’s outer surface. \n(Option can only be applied to Standard Bottom Rail)"]